From e5e77ad2223f662e1615266d8ef39a8db7e65a70 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Felix=20H=C3=A4dicke?= <felixhaedicke@web.de>
Date: Thu, 19 Nov 2020 09:22:32 +0100
Subject: HID: quirks: Add Apple Magic Trackpad 2 to hid_have_special_driver
 list
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

The Apple Magic Trackpad 2 is handled by the magicmouse driver. And
there were severe stability issues when both drivers (hid-generic and
hid-magicmouse) were loaded for this device.

Fixes: https://bugzilla.kernel.org/show_bug.cgi?id=210241

Signed-off-by: Felix Hädicke <felixhaedicke@web.de>
---
 drivers/hid/hid-quirks.c | 2 ++
 1 file changed, 2 insertions(+)

diff --git a/drivers/hid/hid-quirks.c b/drivers/hid/hid-quirks.c
index bf7ecab5d9e5..142e9dae2837 100644
--- a/drivers/hid/hid-quirks.c
+++ b/drivers/hid/hid-quirks.c
@@ -478,6 +478,8 @@ static const struct hid_device_id hid_have_special_driver[] = {
 #if IS_ENABLED(CONFIG_HID_MAGICMOUSE)
 	{ HID_BLUETOOTH_DEVICE(USB_VENDOR_ID_APPLE, USB_DEVICE_ID_APPLE_MAGICMOUSE) },
 	{ HID_BLUETOOTH_DEVICE(USB_VENDOR_ID_APPLE, USB_DEVICE_ID_APPLE_MAGICTRACKPAD) },
+	{ HID_BLUETOOTH_DEVICE(BT_VENDOR_ID_APPLE, USB_DEVICE_ID_APPLE_MAGICTRACKPAD2) },
+	{ HID_USB_DEVICE(USB_VENDOR_ID_APPLE, USB_DEVICE_ID_APPLE_MAGICTRACKPAD2) },
 #endif
 #if IS_ENABLED(CONFIG_HID_MAYFLASH)
 	{ HID_USB_DEVICE(USB_VENDOR_ID_DRAGONRISE, USB_DEVICE_ID_DRAGONRISE_PS3) },
-- 
cgit v1.2.3-1-gf6bb5

From e437ac931e89629f952ce9f3f9dfe45ac505cd0d Mon Sep 17 00:00:00 2001
From: Joshua Ashton <joshua@froggi.es>
Date: Tue, 5 Jan 2021 19:46:01 +0000
Subject: [PATCH] drm/amdgpu: don't limit gtt size on apus

Since commit 24562523688b ("Revert "drm/amd/amdgpu: set gtt size
according to system memory size only""), the GTT size was limited by
3GiB or VRAM size.

This is problematic on APU systems with a small carveout
(notably, those that ship with dGPUs where this is unconfigurable),
where the carveout size can be as low as 128MiB.

This makes it so the GTT size heuristic always uses 3/4ths of
the system memory size on APUs (limiting the size by 3GiB/VRAM size
only on devices with dedicated video memory).

Fixes: 24562523688b ("Revert drm/amd/amdgpu: set gtt size according to
system memory size only")

Signed-off-by: Joshua Ashton <joshua@froggi.es>
---
 drivers/gpu/drm/amd/amdgpu/amdgpu_drv.c |  5 +++--
 drivers/gpu/drm/amd/amdgpu/amdgpu_ttm.c | 12 +++++++++---
 2 files changed, 12 insertions(+), 5 deletions(-)

diff --git a/drivers/gpu/drm/amd/amdgpu/amdgpu_drv.c b/drivers/gpu/drm/amd/amdgpu/amdgpu_drv.c
index 72efd579ec5e..a5a41e9272d6 100644
--- a/drivers/gpu/drm/amd/amdgpu/amdgpu_drv.c
+++ b/drivers/gpu/drm/amd/amdgpu/amdgpu_drv.c
@@ -192,8 +192,9 @@ module_param_named(gartsize, amdgpu_gart_size, uint, 0600);
 
 /**
  * DOC: gttsize (int)
- * Restrict the size of GTT domain in MiB for testing. The default is -1 (It's VRAM size if 3GB < VRAM < 3/4 RAM,
- * otherwise 3/4 RAM size).
+ * Restrict the size of GTT domain in MiB for testing. The default is -1 (On APUs this is 3/4th
+ * of the system memory; on dGPUs this is 3GiB or VRAM sized, whichever is bigger,
+ * with an upper bound of 3/4th of system memory.
  */
 MODULE_PARM_DESC(gttsize, "Size of the GTT domain in megabytes (-1 = auto)");
 module_param_named(gttsize, amdgpu_gtt_size, int, 0600);
diff --git a/drivers/gpu/drm/amd/amdgpu/amdgpu_ttm.c b/drivers/gpu/drm/amd/amdgpu/amdgpu_ttm.c
index 4d8f19ab1014..294f26f4f310 100644
--- a/drivers/gpu/drm/amd/amdgpu/amdgpu_ttm.c
+++ b/drivers/gpu/drm/amd/amdgpu/amdgpu_ttm.c
@@ -1865,9 +1865,15 @@ int amdgpu_ttm_init(struct amdgpu_device *adev)
 		struct sysinfo si;
 
 		si_meminfo(&si);
-		gtt_size = min(max((AMDGPU_DEFAULT_GTT_SIZE_MB << 20),
-			       adev->gmc.mc_vram_size),
-			       ((uint64_t)si.totalram * si.mem_unit * 3/4));
+		gtt_size = (uint64_t)si.totalram * si.mem_unit * 3/4;
+		/* If we have dedicated memory, limit our GTT size to
+		 * 3GiB or VRAM size, whichever is bigger
+		 */
+		if (!(adev->flags & AMD_IS_APU)) {
+			gtt_size = min(max(AMDGPU_DEFAULT_GTT_SIZE_MB << 20,
+				adev->gmc.mc_vram_size),
+				gtt_size);
+		}
 	}
 	else
 		gtt_size = (uint64_t)amdgpu_gtt_size << 20;
-- 
2.30.0

From f7f49141a5dbe9c99d78196b58c44307fb2e6be3 Mon Sep 17 00:00:00 2001
From: Tk-Glitch <ti3nou@gmail.com>
Date: Wed, 3 Feb 2021 11:20:12 +0200
Subject: Revert "cpufreq: Avoid configuring old governors as default with intel_pstate"

This is an undesirable behavior for us since our aggressive ondemand performs
better than schedutil for gaming when using intel_pstate in passive mode.
Also it interferes with the option to select the desired default governor we have.

diff --git a/drivers/cpufreq/Kconfig b/drivers/cpufreq/Kconfig
index 2c7171e0b0010..85de313ddec29 100644
--- a/drivers/cpufreq/Kconfig
+++ b/drivers/cpufreq/Kconfig
@@ -71,7 +71,6 @@ config CPU_FREQ_DEFAULT_GOV_USERSPACE
 
 config CPU_FREQ_DEFAULT_GOV_ONDEMAND
 	bool "ondemand"
-	depends on !(X86_INTEL_PSTATE && SMP)
 	select CPU_FREQ_GOV_ONDEMAND
 	select CPU_FREQ_GOV_PERFORMANCE
 	help
@@ -83,7 +84,6 @@ config CPU_FREQ_DEFAULT_GOV_ONDEMAND
 
 config CPU_FREQ_DEFAULT_GOV_CONSERVATIVE
 	bool "conservative"
-	depends on !(X86_INTEL_PSTATE && SMP)
 	select CPU_FREQ_GOV_CONSERVATIVE
 	select CPU_FREQ_GOV_PERFORMANCE
 	help
